006195 SPE-K33L型落地式站立落座通用三色三工位双轮转丝印机

006195 SPE-K33L floor type stand and sit universal three color three station double wheel screen printing machine

本机用于三色以内T恤或布艺类产品，配置三个独立印刷台位。

This machine is used for printing T-shirt or cloth products within three colors, equipped with three independent printing stations.

本机采用可调节高度架子；可以根据操作者身高和工作习惯调整架子高度；调整范围为台版距离地面58-109厘米；**操作者可根据架子高度站立工作，也可坐在椅子上工作。**

the machine adopts adjustable height rack; The height of the rack can be adjusted according to the operator's height and working habits; The adjustment range from the ground is 58-109 cm ;The operator can work by standing or sitting on a chair according to the height of the rack.

1. 架子底部安装脚轮，可随时移动机器位置；

Casters are installed at the bottom of the rack to move the machine at any time;

1. 整机占地直径160厘米；

The machine covers an area of 160 cm in diameter;

1. 台版与网框部分均可360度任意旋转；

Pallet and screen frame part can be 360 degrees of arbitrary rotation;

1. 网框夹头宽度240毫米，高68毫米，适合网框高度50毫米内的各种网框；

Screen frame clamp width is 240 mm, 68 mm high, suitable for all kinds of screen frame height within50 mm;

1. 夹头均可根据承印物高度进行2厘米高度调整

Clamp can be adjusted by 2cm according to the substrate height .

1. 采用磁铁吸附控制网框抬起平衡。

Using magnet adsorption control screen frame lift balance

8，台版可前后移动100毫米。

The pallet can move backwards or forwards within 10cm(4inch).

006196 SPE-K55L型落地式站立落座通用五色五工位双轮转丝印机

SPE-K55L floor type stand and sit universal five color five station double wheel screen printing machine

本机用于五色以内T恤或布艺类产品，配置五个独立印刷台位。

This machine is used for printing T-shirt or cloth products within five colors, equipped with five independent printing stations.

1. 本机采用可调节高度架子；可以根据操作者身高和工作习惯调整架子高度；调整范围为台版距离地面58-109厘米；

1, the machine adopts adjustable height rack; The height of the rack can be adjusted according to the operator's height and working habits; The adjustment range from the ground is 58-109 cm ;

1. 架子底部安装脚轮，可随时移动机器位置；

Casters are installed at the bottom of the rack to move the machine at any time;

1. 整机占地直径180厘米；

The machine covers an area of 180 cm in diameter;

1. 台版与网框部分均可360度任意旋转；

Pallet and screen frame part can be 360 degrees of arbitrary rotation;

1. 网框夹头宽度240毫米，高68毫米，适合网框高度50毫米内的各种网框；

Screen frame clamp width is 240 mm, 68 mm high, suitable for all kinds of screen frame height within50 mm;

1. 夹头均可根据承印物高度进行2厘米高度调整

Clamp can be adjusted by 2cm according to the substrate height .

1. 采用磁铁吸附控制网框抬起平衡。

Using magnet adsorption control screen frame lift balance.

8，台版可前后移动100毫米。

The pallet can move backwards or forwards within 10cm(4inch).